
Release Notes for XHC MACH3 Ethernet Motion Card

XHC NcEther.dll is the Driver for XHC Ethernet CARD,Used  for MACH3 cnc control system. 
You could control your cnc machine through our Ethernet card.
the card has these feature:
Standard ehternet  Interface
4/6 Axis Step/Direction Output
8 General Purpose Outputs 
16 General Purpose Inputs
1 PWM Output for Spindle Speed Control
Up to 2000Khz Steps pulse

Release Notes: 
2022.5.25 v3.18.0
support EWGP-USB 


2020.12.24 v3.17.0
optimize the ghighspeed function.which is used for g03,ij code. 
2020.12.15 v3.16.9
optimize the communication
2020.9.24 v3.16.8
solve the mach3 command with line start .but return to frist line start problem


2020.9.24 v3.16.7
 solve the device error trigger problem when running


2020.9.8 v3.16.6
modify the thc on function
the thc function is enable only the  thc is on and mach3 is jogging or running g code.
z will go up when thc up signal is actvie.z will dow when thc down signal is active.

2020.7.24 v3.16.5
solve the cannot reset problem when  the active low input io numbers are  more than 8 


2020.5.12 v3.16.4
support g76 code

2020.5.12 v3.16.3
optimize the communication

2019.7.17 v3.16.1
modify whb04bx start/pause function.clear wheel data when reset 



2019.7.8 v3.16
add user self define macro key for whb04bx
2019.1.4 v3.15
modify the function for whb04b

2018.12.19.v3.14
 jog move disable when according limitswitch is on
2018.9.18 v3.13
support the whb04bx.

2018.6.22 V3.12
solve probe maybe change other DRO problem
optimize the second home function
2018.5.9 V3.11
optimize the communication ,make it more stable
2018.1.5 V3.10
change the communication to asyn

2017.11.24 V3.09
solve the second home problem
2017.7.4 V3.08
optimize the communication with card.
1. modify the slave axis home function.
2017.5.5V3.06.1
1. modify the slave axis home function.
2017.4.24 V3.06
1. modity the pwm output with acceleration.
2017.2.15 V3.05
1.modify the single home with backward distance.

2017.2.15 V3.03
solve mach3 g03 command path error when run arc command
2016.11.31 V3.02
solve "device io error" problem
2016.11.31 V3.01
filter the all input io if all zero
modify the plugin windows output io test ,result device communication problem and reset.

2016.9.21 V3.0
release the first version.
this driver is only used for xhc ehternet card.if you want to use our usb card,we could offer it aslo.



Contact Details:
Chengdu XHC Tech., Inc.
 

86-028-81705368 - Sales,Fax
86-028-81701768  - Support

NetWork:
http://www.cdxhctech.com/

517202913@qq.com Support E-mail
QQ:517202913        Support QQ
 
